IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] CBMG5.FGxx.RF.x
[LUMINAIRE] COMO BLACK MELAGENŽ IP44 5 Frosted Glass Faceted Reflector MelaGenŽ ReFresh
[_SEARCH_OPTIC] Direct
[_SEARCH_APPLICATION] Indoor, Direct, Downlight
[_SEARCH_MOUNTING] Ceiling, Recessed
[_SEARCH_CLASSIFICATION] IP20, IP44
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] DLE G1 3030 6V1W 2X6C8B 922
[LAMP] MelaGenŽ ReFresh
[_SEARCH_COLORTEMP] 2200K
[_SEARCH_CRI] 90
[BALLASTCAT] MPQ042 1050/900 220-240Vac 50/60Hz
[BALLAST] 1050mA Tested at 240V 50Hz
[TESTLAB] Architech
[TEST] QA02/17-383IPR
[TESTDATE] 01-APR-2017
[ISSUEDATE] 05-OCT-2021
[_SEARCH_CERTIFICATION] 
TILT=NONE
1 2085 1 19 1 1 2 -0.15 -0.15 0
1 1 40.8
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 
0 
1364.78 1350.44 1307.34 1232.63 1123.44 988.41 836.12 680.95 534.42 408.01 307.43 232.73 172.39 126.42 89.08 57.48 31.6 11.49 0 
