IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] A31.211.114020
[LUMINAIRE] COMO AC 2 Faceted Flat Trim 4000K CRI80
[_SEARCH_OPTIC] Direct
[_SEARCH_APPLICATION] Indoor, Downlight
[_SEARCH_MOUNTING] Ceiling, Recessed
[_SEARCH_CLASSIFICATION] IP20
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] DLE-G2-LES65-2000-840
[LAMP] 4000K CRI80 LED Module Tested @ 230V 50Hz
[_SEARCH_COLORTEMP] 4000K
[_SEARCH_CRI] 80
[TESTLAB] Architech
[TEST] QA02/17-50I
[TESTDATE] 01-APR-2017
[ISSUEDATE] 01-OCT-2017
[_SEARCH_CERTIFICATION] 
TILT=NONE
1 1611 1 19 1 1 2 -0.15 -0.15 0
1 1 22.5
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 
0 
1226 1269 1310 1317 1241 1091 907 619 365 180 79 47 32 22 15 9 6 4 1 
