IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] CBP4.FG.xx3090.x
[LUMINAIRE] COMO BLACK PLUS IP44 4 Frosted Glass Faceted Reflector 3000K CRI Ra90
[_SEARCH_OPTIC] Direct
[_SEARCH_APPLICATION] Indoor, Direct, Downlight
[_SEARCH_MOUNTING] Ceiling, Recessed
[_SEARCH_CLASSIFICATION] IP20, IP44
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] DLE G1 3030 930
[LAMP] 3000K CRI Ra90 LED Module
[_SEARCH_COLORTEMP] 3000K
[_SEARCH_CRI] 90
[BALLASTCAT] MPQ034 850/700 220-240V~ 50Hz/60Hz
[BALLAST] 700mA Tested at 240 V 50 Hz
[TESTLAB] Architech
[TEST] QA02/17-383IPR
[TESTDATE] 01-APR-2017
[ISSUEDATE] 01-SEP-2021
[_SEARCH_CERTIFICATION] 
TILT=NONE
1 2224 1 19 1 1 2 -0.15 -0.15 0
1 1 26.1
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 
0 
1455.32 1440.02 1394.07 1314.4 1197.97 1053.98 891.58 726.12 569.87 435.07 327.83 248.17 183.83 134.8 94.99 61.29 33.7 12.26 0 
