IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] CB4.971.xx4080.x
[LUMINAIRE] COMO BLACK IP44 4 Frosted Glass Faceted Reflector 4000K CRI80
[_SEARCH_OPTIC] Direct
[_SEARCH_APPLICATION] Indoor, Direct, Downlight
[_SEARCH_MOUNTING] Ceiling, Recessed
[_SEARCH_CLASSIFICATION] IP20, IP44
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] DLE G1 2835 9V1W 4C15B 840
[LAMP] 4000K CRI80 LED Module
[_SEARCH_COLORTEMP] 4000K
[_SEARCH_CRI] 80
[BALLASTCAT] MPQ034 850/700 220-240V~ 50Hz/60Hz
[BALLAST] 700mA Tested at 240 V 50 Hz
[TESTLAB] Architech
[TEST] QA02/17-383IPR
[TESTDATE] 01-APR-2017
[ISSUEDATE] 19-SEP-2019
[_SEARCH_CERTIFICATION] 
TILT=NONE
1 2329 1 19 1 1 2 -0.15 -0.15 0
1 1 27.5
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 
0 
1524.11 1508.07 1459.94 1376.5 1254.58 1103.77 933.72 760.45 596.81 455.63 343.33 259.91 192.52 141.18 99.47 64.17 35.29 12.84 0 
