IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] CBP5.FG.xx3090.x
[LUMINAIRE] COMO BLACK PLUS IP44 5 Frosted Glass Faceted Reflector 3000K CRI Ra90
[_SEARCH_OPTIC] Direct
[_SEARCH_APPLICATION] Indoor, Direct, Downlight
[_SEARCH_MOUNTING] Ceiling, Recessed
[_SEARCH_CLASSIFICATION] IP20, IP44
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] DLE G1 3030 930
[LAMP] 3000K CRI Ra90 LED Module
[_SEARCH_COLORTEMP] 3000K
[_SEARCH_CRI] 90
[BALLASTCAT] MPQ042 1050/900 220-240V~ 50Hz/60Hz
[BALLAST] 1050mA Tested at 240 V 50 Hz
[TESTLAB] Architech
[TEST] QA02/17-383IPR
[TESTDATE] 01-APR-2017
[ISSUEDATE] 01-SEP-2021
[_SEARCH_CERTIFICATION] 
TILT=NONE
1 3337 1 19 1 1 2 -0.15 -0.15 0
1 1 37.7
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 
0 
2183.67 2160.73 2091.76 1972.24 1797.53 1581.48 1337.81 1089.52 855.09 652.83 491.9 372.37 275.83 202.27 142.53 91.96 50.57 18.39 0 
