IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] CBMG4.FGxx.RF.x
[LUMINAIRE] COMO BLACK MELAGENŽ IP44 4 Frosted Glass Faceted Reflector MelaGenŽ ReFresh
[_SEARCH_OPTIC] Direct
[_SEARCH_APPLICATION] Indoor, Direct, Downlight
[_SEARCH_MOUNTING] Ceiling, Recessed
[_SEARCH_CLASSIFICATION] IP20, IP44
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] DLE G1 3030 6V1W 2X6C8B 922
[LAMP] MelaGenŽ ReFresh
[_SEARCH_COLORTEMP] 2200K
[_SEARCH_CRI] 90
[BALLASTCAT] MPQ034 850/700 220-240Vac 50/60Hz
[BALLAST] 700mA Tested at 240V 50Hz
[TESTLAB] Architech
[TEST] QA02/17-383IPR
[TESTDATE] 01-APR-2017
[ISSUEDATE] 05-OCT-2021
[_SEARCH_CERTIFICATION] 
TILT=NONE
1 1389 1 19 1 1 2 -0.15 -0.15 0
1 1 27.5
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 
0 
908.81 899.26 870.56 820.81 748.1 658.18 556.77 453.44 355.87 271.69 204.72 154.97 114.8 84.18 59.32 38.28 21.04 7.65 0 
