IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] CBMG2.DGxx.RF.x
[LUMINAIRE] COMO BLACK MELAGEN® DÉCOR 2 Décor Glass Faceted Reflector MelaGen® ReFresh
[_SEARCH_OPTIC] Direct
[_SEARCH_APPLICATION] Indoor, Direct-Indirect, Downlight
[_SEARCH_MOUNTING] Ceiling, Recessed
[_SEARCH_CLASSIFICATION] IP20
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] DLE G1 3030 6V1W 2X6C8B 922
[LAMP] MelaGen® ReFresh
[_SEARCH_COLORTEMP] 2200K
[_SEARCH_CRI] 90
[BALLASTCAT] MPQ015 350/180 220-240Vac 50/60Hz
[BALLAST] 350mA Tested at 240V 50Hz
[TESTLAB] Architech
[TEST] QA02/17-47IPR
[TESTDATE] 01-APR-2017
[ISSUEDATE] 05-OCT-2021
[_SEARCH_CERTIFICATION] 
TILT=NONE
1 786 1 37 1 1 2 -0.21 -0.21 0.01
1 1 13.9
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 95 100 105 110 115 120 125 130 135 140 145 150 155 160 165 170 175 180 
0 
535.11 552.78 566.52 572.9 547.86 494.36 409.43 273.44 166.42 85.81 37.86 30.28 25.23 20.18 15.14 12.62 10.1 6.56 2.53 3.78 5.05 6.31 7.58 8.83 10.1 8.83 7.58 6.31 5.05 3.78 2.53 1.26 0 0 0 0 0 
