IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] CBMG2.FGxx.BL.x
[LUMINAIRE] COMO BLACK MELAGENŽ IP44 2 Frosted Glass Faceted Reflector MelaGenŽ Blue
[_SEARCH_OPTIC] Direct
[_SEARCH_APPLICATION] Indoor, Direct, Downlight
[_SEARCH_MOUNTING] Ceiling, Recessed
[_SEARCH_CLASSIFICATION] IP20, IP44
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] DLE G1 3030 6V1W 2X6C8B 942
[LAMP] MelaGenŽ Blue
[_SEARCH_COLORTEMP] 4200K
[_SEARCH_CRI] 90
[BALLASTCAT] MPQ015 350/180 220-240Vac 50/60Hz
[BALLAST] 350mA Tested at 240V 50Hz
[TESTLAB] Architech
[TEST] QA02/17-383IPR
[TESTDATE] 01-APR-2017
[ISSUEDATE] 05-OCT-2021
[_SEARCH_CERTIFICATION] 
TILT=NONE
1 920 1 19 1 1 2 -0.15 -0.15 0
1 1 13.9
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 
0 
602.41 596.07 577.05 544.07 495.88 436.27 369.06 300.57 235.9 180.09 135.7 102.73 76.09 55.81 39.32 25.37 13.95 5.07 0 
