IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] CB2.971.xx4080.x
[LUMINAIRE] COMO BLACK IP44 2 Frosted Glass Faceted Reflector 4000K CRI80
[_SEARCH_OPTIC] Direct
[_SEARCH_APPLICATION] Indoor, Direct, Downlight
[_SEARCH_MOUNTING] Ceiling, Recessed
[_SEARCH_CLASSIFICATION] IP20, IP44
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] DLE G1 2835 9V1W 4C15B 840
[LAMP] 4000K CRI80 LED Module
[_SEARCH_COLORTEMP] 4000K
[_SEARCH_CRI] 80
[BALLASTCAT] MPQ015 350/180 220-240V~ 50Hz/60Hz
[BALLAST] 350mA Tested at 240 V 50 Hz
[TESTLAB] Architech
[TEST] QA02/17-383IPR
[TESTDATE] 01-APR-2017
[ISSUEDATE] 19-SEP-2019
[_SEARCH_CERTIFICATION] 
TILT=NONE
1 1235 1 19 1 1 2 -0.15 -0.15 0
1 1 13.9
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 
0 
808.6 800.1 774.56 730.3 665.61 585.6 495.38 403.45 316.64 241.73 182.15 137.89 102.14 74.91 52.78 34.05 18.72 6.81 0 
