IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] CBP1.FG.xx3090.x
[LUMINAIRE] COMO BLACK PLUS IP44 1 Frosted Glass Faceted Reflector 3000K CRI Ra90
[_SEARCH_OPTIC] Direct
[_SEARCH_APPLICATION] Indoor, Direct, Downlight
[_SEARCH_MOUNTING] Ceiling, Recessed
[_SEARCH_CLASSIFICATION] IP20, IP44
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] DLE G1 3030 930
[LAMP] 3000K CRI Ra90 LED Module
[_SEARCH_COLORTEMP] 3000K
[_SEARCH_CRI] 90
[BALLASTCAT] MPQ015 350/180 220-240V~ 50Hz/60Hz
[BALLAST] 180mA Tested at 240 V 50 Hz
[TESTLAB] Architech
[TEST] QA02/17-383IPR
[TESTDATE] 01-APR-2017
[ISSUEDATE] 01-SEP-2021
[_SEARCH_CERTIFICATION] 
TILT=NONE
1 572 1 19 1 1 2 -0.15 -0.15 0
1 1 8.9
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 
0 
374.59 370.65 358.82 338.32 308.34 271.29 229.48 186.9 146.68 111.98 84.38 63.88 47.32 34.7 24.45 15.77 8.68 3.15 0 
