IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] CBMG2.FGxx.RF.x
[LUMINAIRE] COMO BLACK MELAGENŽ IP44 2 Frosted Glass Faceted Reflector MelaGenŽ ReFresh
[_SEARCH_OPTIC] Direct
[_SEARCH_APPLICATION] Indoor, Direct, Downlight
[_SEARCH_MOUNTING] Ceiling, Recessed
[_SEARCH_CLASSIFICATION] IP20, IP44
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] DLE G1 3030 6V1W 2X6C8B 922
[LAMP] MelaGenŽ ReFresh
[_SEARCH_COLORTEMP] 2200K
[_SEARCH_CRI] 90
[BALLASTCAT] MPQ015 350/180 220-240Vac 50/60Hz
[BALLAST] 350mA Tested at 240V 50Hz
[TESTLAB] Architech
[TEST] QA02/17-383IPR
[TESTDATE] 01-APR-2017
[ISSUEDATE] 05-OCT-2021
[_SEARCH_CERTIFICATION] 
TILT=NONE
1 696 1 19 1 1 2 -0.15 -0.15 0
1 1 13.9
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 
0 
455.42 450.63 436.25 411.32 374.88 329.83 279.01 227.23 178.34 136.15 102.58 77.66 57.53 42.18 29.72 19.18 10.54 3.83 0 
