IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] A31.211.114010
[LUMINAIRE] COMO AC 1 Faceted Flat Trim 4000K CRI80
[_SEARCH_OPTIC] Direct
[_SEARCH_APPLICATION] Indoor, Downlight
[_SEARCH_MOUNTING] Ceiling, Recessed
[_SEARCH_CLASSIFICATION] IP20
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] DLE-G2-LES65-1100-840
[LAMP] 4000K CRI80 LED Module Tested @ 230V 50Hz
[_SEARCH_COLORTEMP] 4000K
[_SEARCH_CRI] 80
[TESTLAB] Architech
[TEST] QA02/17-51I
[TESTDATE] 01-APR-2017
[ISSUEDATE] 01-OCT-2017
[_SEARCH_CERTIFICATION] 
TILT=NONE
1 843 1 19 1 1 2 -0.15 -0.15 0
1 1 11.5
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 
0 
661 677 701 706 664 578 474 314 187 91 39 23 15 11 7 5 3 2 0 
