IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] CBP4.FG.xx4090.x
[LUMINAIRE] COMO BLACK PLUS IP44 4 Frosted Glass Faceted Reflector 4000K CRI Ra90
[_SEARCH_OPTIC] Direct
[_SEARCH_APPLICATION] Indoor, Direct, Downlight
[_SEARCH_MOUNTING] Ceiling, Recessed
[_SEARCH_CLASSIFICATION] IP20, IP44
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] DLE G1 3030 940
[LAMP] 4000K CRI Ra90 LED Module
[_SEARCH_COLORTEMP] 4000K
[_SEARCH_CRI] 90
[BALLASTCAT] MPQ034 850/700 220-240V~ 50Hz/60Hz
[BALLAST] 700mA Tested at 240 V 50 Hz
[TESTLAB] Architech
[TEST] QA02/17-383IPR
[TESTDATE] 01-APR-2017
[ISSUEDATE] 01-SEP-2021
[_SEARCH_CERTIFICATION] 
TILT=NONE
1 2502 1 19 1 1 2 -0.15 -0.15 0
1 1 27
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 
0 
1637.32 1620.09 1568.39 1478.75 1347.77 1185.76 1003.08 816.94 641.14 489.47 368.83 279.22 206.82 151.67 106.86 68.94 37.91 13.79 0 
