IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] A31.271.113020
[LUMINAIRE] COMO AC 2 Faceted Beveled Trim c/w Clear Glass 3000K CRI80
[_SEARCH_OPTIC] Direct
[_SEARCH_APPLICATION] Indoor, Downlight
[_SEARCH_MOUNTING] Ceiling, Recessed
[_SEARCH_CLASSIFICATION] IP44
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] DLE-G2-LES65-2000-830
[LAMP] 3000K CRI80 LED Module Tested @ 230V 50Hz
[_SEARCH_COLORTEMP] 3000K
[_SEARCH_CRI] 80
[TESTLAB] Architech
[TEST] QA02/17-47I
[TESTDATE] 01-APR-2017
[ISSUEDATE] 01-OCT-2017
[_SEARCH_CERTIFICATION] 
TILT=NONE
1 1341 1 19 1 1 2 -0.15 -0.15 0
1 1 22.5
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 
0 
1018.39 1050.56 1087.32 1096.51 1034.01 909.01 756.44 514.71 303.31 149.82 66.18 39.52 26.66 18.38 12.87 9.19 4.6 2.76 0 
