IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] 10517100-500mA
[LUMINAIRE] MARTINA MINI 30° 500mA 4000K
[_SEARCH_APPLICATION] Indoor, Outdoor, Area, Direct, Flood, Security
[_SEARCH_MOUNTING] Ceiling, Floor, Ground, Wall, Surface
[_SEARCH_CLASSIFICATION] IP67, IK05
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] LA0216/17
[LAMP] LED
[_SEARCH_COLORTEMP] 4000K
[_SEARCH_CRI] 80
[TEST] ART.1058700 500mA*
[_SEARCH_CERTIFICATION] 
[ISSUEDATE] 23-MAR-2020
TILT=NONE
1 129 1 19 1 1 2 -0.044 -0.044 0
1 1 1.6
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 
0 
355.65 334.59 267.01 178.77 103.24 54.08 28.5 16.16 10.09 6.78 4.91 3.64 2.69 1.94 1.26 0.68 0.26 0.08 0.03 
