IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] 10514420-500mA
[LUMINAIRE] MARTINA MINI 30° 500mA 2700K
[_SEARCH_APPLICATION] Indoor, Outdoor, Area, Direct, Flood, Security
[_SEARCH_MOUNTING] Ceiling, Floor, Ground, Wall, Surface
[_SEARCH_CLASSIFICATION] IP67, IK05
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] LA0217/17
[LAMP] LED
[_SEARCH_COLORTEMP] 2700K
[_SEARCH_CRI] 80
[TEST] ART.1058700 500mA*
[_SEARCH_CERTIFICATION] 
[ISSUEDATE] 23-MAR-2020
TILT=NONE
1 111 1 19 1 1 2 -0.044 -0.044 0
1 1 1.6
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 
0 
306.02 287.91 229.75 153.83 88.84 46.54 24.52 13.91 8.68 5.84 4.23 3.13 2.32 1.67 1.08 0.59 0.22 0.07 0.03 
