IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] CBMG4.FGxx.BL.x
[LUMINAIRE] COMO BLACK MELAGENŽ IP44 4 Frosted Glass Faceted Reflector MelaGenŽ Blue
[_SEARCH_OPTIC] Direct
[_SEARCH_APPLICATION] Indoor, Direct, Downlight
[_SEARCH_MOUNTING] Ceiling, Recessed
[_SEARCH_CLASSIFICATION] IP20, IP44
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] DLE G1 3030 6V1W 2X6C8B 942
[LAMP] MelaGenŽ Blue
[_SEARCH_COLORTEMP] 4200K
[_SEARCH_CRI] 90
[BALLASTCAT] MPQ034 850/700 220-240Vac 50/60Hz
[BALLAST] 700mA Tested at 240V 50Hz
[TESTLAB] Architech
[TEST] QA02/17-383IPR
[TESTDATE] 01-APR-2017
[ISSUEDATE] 05-OCT-2021
[_SEARCH_CERTIFICATION] 
TILT=NONE
1 1840 1 19 1 1 2 -0.15 -0.15 0
1 1 27.5
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 
0 
1204.05 1191.38 1153.35 1087.44 991.12 871.98 737.64 600.76 471.48 359.95 271.23 205.33 152.09 111.53 78.58 50.69 27.88 10.14 0 
