IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] CBMG3.DGxx.RF.x
[LUMINAIRE] COMO BLACK MELAGEN® DÉCOR 3 Décor Glass Faceted Reflector MelaGen® ReFresh
[_SEARCH_OPTIC] Direct
[_SEARCH_APPLICATION] Indoor, Direct-Indirect, Downlight
[_SEARCH_MOUNTING] Ceiling, Recessed
[_SEARCH_CLASSIFICATION] IP20
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] DLE G1 3030 6V1W 2X6C8B 922
[LAMP] MelaGen® ReFresh
[_SEARCH_COLORTEMP] 2200K
[_SEARCH_CRI] 90
[BALLASTCAT] MPQ024 600/450 220-240Vac 50/60Hz
[BALLAST] 500mA Tested at 240V 50Hz
[TESTLAB] Architech
[TEST] QA02/17-47IPR
[TESTDATE] 01-APR-2017
[ISSUEDATE] 05-OCT-2021
[_SEARCH_CERTIFICATION] 
TILT=NONE
1 1121 1 37 1 1 2 -0.21 -0.21 0.01
1 1 20.9
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 95 100 105 110 115 120 125 130 135 140 145 150 155 160 165 170 175 180 
0 
763.47 788.69 808.28 817.39 781.67 705.32 584.15 390.14 237.44 122.43 54.01 43.21 36 28.8 21.61 18.01 14.41 9.36 3.6 5.4 7.2 9 10.81 12.6 14.41 12.6 10.81 9 7.2 5.4 3.6 1.79 0 0 0 0 0 
