IESNA:LM-63-2002
[MANUFAC] Versalux Lighting Systems Pty Ltd
[LUMCAT] CBMG1.DGxx.RF.x
[LUMINAIRE] COMO BLACK MELAGEN® DÉCOR 1 Décor Glass Faceted Reflector MelaGen® ReFresh
[_SEARCH_OPTIC] Direct
[_SEARCH_APPLICATION] Indoor, Direct-Indirect, Downlight
[_SEARCH_MOUNTING] Ceiling, Recessed
[_SEARCH_CLASSIFICATION] IP20
[_SEARCH_SOURCETYPE] LED
[LAMPCAT] DLE G1 3030 6V1W 2X6C8B 922
[LAMP] MelaGen® ReFresh
[_SEARCH_COLORTEMP] 2200K
[_SEARCH_CRI] 90
[BALLASTCAT] MPQ015 350/180 220-240Vac 50/60Hz
[BALLAST] 180mA Tested at 240V 50Hz
[TESTLAB] Architech
[TEST] QA02/17-47IPR
[TESTDATE] 01-APR-2017
[ISSUEDATE] 05-OCT-2021
[_SEARCH_CERTIFICATION] 
TILT=NONE
1 404 1 37 1 1 2 -0.21 -0.21 0.01
1 1 7.8
0 5 10 15 20 25 30 35 40 45 50 55 60 65 70 75 80 85 90 95 100 105 110 115 120 125 130 135 140 145 150 155 160 165 170 175 180 
0 
274.89 283.97 291.02 294.3 281.44 253.95 210.33 140.47 85.49 44.08 19.45 15.56 12.96 10.37 7.78 6.48 5.19 3.37 1.3 1.94 2.6 3.24 3.89 4.53 5.19 4.53 3.89 3.24 2.6 1.94 1.3 0.65 0 0 0 0 0 
